GSIC - Global Service Information Center

# A750F AUTOMATIC TRANSMISSION > TORQUE SPECIFICATIONS

Automatic Transmission Assembly
Part tightened | N*m | kgf*cm | ft.*lbf
Park/neutral position switch Bolt | 13 | 130 | 9
Park/neutral position switch Nut | 6.9 | 70 | 61 in.*lbf
Transmission control cable x Automatic transmission | 14 | 143 | 10
Engine mounting insulator rear No.1 x Automatic transmission | 65 | 663 | 48
Automatic transmission x Engine (17 mm head) | 71 | 720 | 53
Automatic transmission x Engine (14 mm head) | 37 | 380 | 27
Torque converter clutch x Drive plate | 48 | 490 | 35
Engine rear mounting member x Body Nut | 72 | 735 | 53
Transmission control cable bracket No.1 x Automatic transmission | 14 | 143 | 10
Oil cooler tube clamp | 5 | 51 | 43 in.*lbf
Oil cooler tube outlet x Automatic transmission | 34 | 346 | 25
Oil cooler tube inlet x Automatic transmission | 34 | 346 | 25
Exhaust pipe x Exhaust manifold | 62 | 630 | 46
Exhaust pipe x Exhaust pipe | 48 | 490 | 35
Speed sensor x Automatic transmission | 5.4 | 55 | 48 in.*lbf
Drain plug x Oil pan | 28 | 285 | 21
Transmission wire set bolt x Automatic transmission | 5.4 | 55 | 48 in.*lbf
Transmission wire clamp x Valve body (A) | 11 | 110 | 8
Transmission wire clamp x Valve body (B) | 10 | 100 | 7
Oil strainer x Valve body | 10 | 100 | 7
Oil pan x Transmission case | 4.4 | 45 | 39 in.*lbf
Shift solenoid valve S1 x Valve body | 6.4 | 65 | 56 in.*lbf
Shift solenoid valve S2 x Valve body | 10 | 100 | 7
Shift solenoid valve SR x Valve body | 6.4 | 65 | 56 in.*lbf
Shift solenoid valve SLU, SL2 x Valve body | 6.4 | 65 | 56 in.*lbf
Shift solenoid valve SLT, SL1 x Valve body | 6.4 | 65 | 56 in.*lbf
Valve body x Transmission case | 11 | 110 | 8
Floor shift assembly x Body | 14 | 143 | 10
Overflow plug x Automatic transmission | 20 | 204 | 15
Refill plug x Automatic transmission | 39 | 400 | 29
Wire harness x Automatic transmission | 8.0 | 83 | 71 in.*lbf
Transmission control cable assembly x Body | 5.5 | 56 | 49 in.*lbf
Frame crossmember x Body | 50 | 510 | 37
Frame crossmember x Engine mounting insulator rear | 27 | 275 | 20
Engine mounting insulator rear x Automatic transmission | 65 | 663 | 48