GSIC - Global Service Information Center

### WATER PUMP > INSTALLATION

1. INSTALL WATER PUMP ASSEMBLY

2. INSTALL V-RIBBED BELT TENSIONER ASSEMBLY

3. INSTALL GENERATOR ASSEMBLY

4. INSTALL NO. 2 IDLER PULLEY SUB-ASSEMBLY

5. INSTALL WATER INLET HOUSING

6. CONNECT RADIATOR HOSE INLET

7. CONNECT RADIATOR HOSE OUTLET

8. INSTALL AIR CLEANER ASSEMBLY

9. CONNECT NO. 2 VENTILATION HOSE

10. INSTALL FAN SHROUD

11. CONNECT CABLE TO NEGATIVE BATTERY TERMINAL

12. ADD ENGINE COOLANT

13. CHECK FOR ENGINE COOLANT LEAKS

14. INSTALL V-BANK COVER

15. INSTALL NO. 1 ENGINE UNDER COVER

16. PERFORM INITIALIZATION