GSIC - Global Service Information Center

### AUDIO AND VISUAL SYSTEM > Illumination for Panel Switch does not Come on with Tail Switch ON

## for Preparation Click here

## INSPECTION PROCEDURE

1.INSPECT NIGHTTIME ILLUMINATION

1. Turn on the light control switch and check the nighttime illumination of the vehicle interior.

   Result
   Result | Proceed to
   Only radio receiver nighttime illumination does not activate | A
   No nighttime illumination at all | B

| B |

GO TO COMBINATION METER

A |

PROCEED TO NEXT CIRCUIT INSPECTION SHOWN IN PROBLEM SYSTEM TABLE