GSIC - Global Service Information Center

# METER / GAUGE SYSTEM > DATA LIST / ACTIVE TEST

## for Preparation Click here

READ DATA LIST

HINT:

  Using the intelligent tester Data List allows switch, actuator and other item values to be read without removing any parts. Reading the Data List early in troubleshooting is one way to save time.

1. Connect the intelligent tester to the DLC3.

2. Turn the ignition switch ON.

3. Read the Data List according to the display on the tester.

   Skid control ECU with actuator
   Item | Measurement Item / Display (Range) | Normal Condition | Diagnostic Note
   Parking Brake SW | Parking brake switch/ ON or OFF | ON: Parking brake is applied OFF: Parking brake is not applied | -

PERFORM ACTIVE TEST

HINT:

  Performing the intelligent tester Active Test allows relay, VSV, actuator and other items to be operated without removing any parts. Performing the Active Test early in troubleshooting is one way to save time. The Data List can be displayed during the Active Test.

1. Connect the intelligent tester to the DLC3.

2. Turn the ignition switch ON.

3. Perform the Active Test according to the display on the tester.

   Skid control ECU with actuator
   Item | Test Details | Diagnostic Note
   ABS Warning Light | ABS warning light/ ON or OFF | -