GSIC - Global Service Information Center

# SEAT BELT > TORQUE SPECIFICATIONS

FRONT SEAT BELT
Part Tightened | N*m | kgf*cm | ft.*lbf
Extra cab and double cab Front shoulder belt anchor adjuster assembly x Body | 42 | 428 | 31
w/o Pretensioner Single cab and extra cab Front seat outer belt assembly retractor) x Body | 42 | 428 | 31
w/o Pretensioner Double cab Front seat outer belt assembly (Upper part of retractor) x Body | 4.8 | 49 | 42 in.*lbf
w/ Pretensioner Front seat outer belt assembly (Upper part of retractor) x Body | 4.8 | 49 | 42 in.*lbf
w/ Pretensioner Front seat outer belt assembly (Lower part of retractor) x Body | 42 | 428 | 31
Single cab Front seat outer belt assembly (shoulder anchor) x Body | 42 | 428 | 31
Extra cab and double cab Front seat outer belt assembly (shoulder anchor) x Front shoulder belt anchor adjuster assembly | 42 | 428 | 31
Front seat outer belt assembly (floor anchor) x Body | 42 | 428 | 31

REAR SEAT
Part Tightened | N*m | kgf*cm | ft.*lbf
Double cab Rear No. 1 seat belt assembly inner LH (floor anchor) x Body | 42 | 428 | 31
Double cab Rear No. 1 seat belt assembly inner RH (floor anchor) x Body | 42 | 428 | 31
Extra cab Rear No. 1 seat belt assembly inner (floor anchor) x Body | 42 | 428 | 31
Double cab Rear seat outer belt assembly (retractor) x Body | 42 | 428 | 31
Extra cab Rear seat outer belt assembly (Upper part of retractor) x Body | 4.8 | 49 | 42 in.*lbf
Rear seat outer belt assembly (shoulder anchor) x Body | 42 | 428 | 31
Extra cab rear seat outer belt assembly (floor anchor) x Body | 42 | 428 | 31