GSIC - Global Service Information Center

### DTC 62-47 CD Temperature is High (AUDIO H/U)

## for Preparation Click here

## DESCRIPTION

DTC No. | DTC Detection Condition | Trouble Area
62-47 | High temperature is detected in CD player. | Radio receiver assembly

## INSPECTION PROCEDURE

1.CHECK RADIO RECEIVER ASSEMBLY

1. With the ignition switch OFF, leave vehicle the in a cool, shaded place.

1. When the temperature of the radio receiver assembly has returned to normal, turn the ignition switch to ACC.

1. Check for DTCs again.

   OK:
     No DTC is output.

| NG |

REPLACE RADIO RECEIVER ASSEMBLY

OK |

END