GSIC - Global Service Information Center

### REAR LEAF SPRING (for 4WD) > INSTALLATION

1. INSTALL REAR LH LEAF SPRING ASSEMBLY

2. INSTALL NO. 2 REAR LEAF SPRING SHACKLE SUB-ASSEMBLY

3. TEMPORARILY INSTALL LEAF SPRING SHACKLE INNER PLATE

4. TEMPORARILY INSTALL REAR LEAF SPRING PIN BOLT

5. TEMPORARILY INSTALL REAR LEAF SPRING U BOLT

6. INSTALL REAR SHOCK ABSORBER ASSEMBLY

7. INSTALL NO. 3 PARKING BRAKE CABLE ASSEMBLY

8. STABILIZE SUSPENSION

9. TIGHTEN LEAF SPRING SHACKLE INNER PLATE NUT

10. TIGHTEN REAR LEAF SPRING PIN NUT

11. TIGHTEN LEAF SPRING U BOLT SEAT NUT

12. INSTALL REAR WHEEL