GSIC - Global Service Information Center

# 2KD-FTV EXHAUST > TORQUE SPECIFICATIONS

Part Tightened | N*m | kgf*cm | ft.*lbf
Front exhaust pipe assembly x Outlet pipe | 43 | 438 | 32
Center exhaust pipe assembly x Front exhaust pipe assembly | 48 | 489 | 35
Tailpipe assembly x Center exhaust pipe assembly | 48 | 489 | 35
Front floor No. 1 heat insulator x Body | 5.0 | 51 | 44 in.*lbf
Rear floor rear heat insulator x Body | 5.0 | 51 | 44 in.*lbf
Main muffler heat insulator x Body | 5.0 | 51 | 44 in.*lbf