GSIC - Global Service Information Center

# AIR CONDITIONING > TORQUE SPECIFICATIONS

REFRIGERANT LINE:

  Part Tightened | N*m | kgf*cm | ft.*lbf
  Air conditioning tube and accessory assembly x Cooler condenser assembly | 5.4 | 55 | 48 in.*lbf
  No. 1 cooler refrigerant discharge hose x Cooler condenser assembly | 5.4 | 55 | 48 in.*lbf
  Air conditioning tube and accessory assembly x Cooler expansion valve | 5.4 | 55 | 48 in.*lbf
  Air conditioning tube and accessory assembly x vehicle body | 5.4 | 55 | 48 in.*lbf
  Suction pipe sub-assembly x Cooler compressor assembly | 9.8 | 100 | 7
  No. 1 cooler refrigerant discharge hose x Cooler compressor assembly | 9.8 | 100 | 7

AIR CONDITIONING AND BLOWER UNIT:

  Part Tightened | N*m | kgf*cm | ft.*lbf
  Instrument panel reinforcement assembly x Body | 20 | 204 | 15
  Instrument panel reinforcement assembly x Brake pedal support sub-assembly | 18 | 184 | 13
  Air conditioning and blower assembly x Instrument panel reinforcement assembly | 9.8 | 100 | 7
  Air conditioning and blower assembly x body | 9.8 | 100 | 7
  No. 1 instrument panel brace sub-assembly x Air conditioning and blower assembly | 9.8 | 100 | 7

AIR CONDITIONING UNIT:

  Part Tightened | N*m | kgf*cm | ft.*lbf
  Instrument panel reinforcement assembly x Body | 20 | 204 | 15
  Instrument panel reinforcement assembly x Brake pedal support sub-assembly | 18 | 184 | 13
  Air conditioning unit x Instrument panel reinforcement assembly | 9.8 | 100 | 7
  Air conditioning unit x body | 9.8 | 100 | 7
  No. 1 instrument panel brace sub-assembly x Air conditioning unit | 9.8 | 100 | 7
  Cooler expansion valve x No. 1 cooler evaporator sub-assembly | 3.5 | 35 | 30 in.*lbf

BLOWER UNIT:

  Part Tightened | N*m | kgf*cm | ft.*lbf
  Instrument panel reinforcement assembly x Body | 20 | 204 | 15
  Instrument panel reinforcement assembly x Brake pedal support sub-assembly | 18 | 184 | 13
  No. 1 instrument panel brace sub-assembly x Air conditioning unit | 9.8 | 100 | 7
  Blower assembly x body | 9.8 | 100 | 7

1TR-FE COMPRESSOR AND PULLEY:

  Part Tightened | N*m | kgf*cm | ft.*lbf
  Cooler compressor assembly x Engine | 24.5 | 250 | 18
  Suction hose sub-assembly x Cooler compressor assembly | 9.8 | 100 | 7
  No. 1 cooler refrigerant discharge hose x Cooler compressor assembly | 9.8 | 100 | 7

2TR-FE COMPRESSOR AND PULLEY:

  Part Tightened | N*m | kgf*cm | ft.*lbf
  Cooler compressor assembly x Engine | 24.5 | 250 | 18
  Suction hose sub-assembly x Cooler compressor assembly | 9.8 | 100 | 7
  No. 1 cooler refrigerant discharge hose x Cooler compressor assembly | 9.8 | 100 | 7

2KD-FTV COMPRESSOR AND PULLEY:

  Part Tightened | N*m | kgf*cm | ft.*lbf
  Cooler compressor assembly x Engine | 24.5 | 250 | 18
  Suction hose sub-assembly x Cooler compressor assembly | 9.8 | 100 | 7
  No. 1 cooler refrigerant discharge hose x Cooler compressor assembly | 9.8 | 100 | 7

1TR-FE CONDENSER:

  Part Tightened | N*m | kgf*cm | ft.*lbf
  Cooler condenser assembly x Radiator support upper | 5.4 | 55 | 47 in.*lbf
  Radiator support upper x Radiator support side | 5.5 | 56 | 49 in.*lbf
  Hood lock assembly x Radiator support upper | 8.0 | 82 | 71 in.*lbf
  Air conditioning tube and accessory assembly x Cooler condenser assembly | 5.4 | 55 | 47 in.*lbf
  No. 1 cooler refrigerant discharge hose x Cooler condenser assembly | 5.4 | 55 | 47 in.*lbf

2TR-FE CONDENSER:

  Part Tightened | N*m | kgf*cm | ft.*lbf
  Cooler condenser assembly x Radiator support upper | 5.4 | 55 | 47 in.*lbf
  Radiator support upper x Radiator support side | 5.5 | 56 | 49 in.*lbf
  Hood lock assembly x Radiator support upper | 8.0 | 82 | 71 in.*lbf
  Air conditioning tube and accessory assembly x Cooler condenser assembly | 5.4 | 55 | 47 in.*lbf
  No. 1 cooler refrigerant discharge hose x Cooler condenser assembly | 5.4 | 55 | 47 in.*lbf

2KD-FTV CONDENSER:

  Part Tightened | N*m | kgf*cm | ft.*lbf
  Cooler condenser assembly x Radiator support upper | 5.4 | 55 | 47 in.*lbf
  Radiator support upper x Radiator support side | 5.5 | 56 | 49 in.*lbf
  Hood lock assembly x Radiator support upper | 8.0 | 82 | 71 in.*lbf
  Air conditioning tube and accessory assembly x Cooler condenser assembly | 5.4 | 55 | 47 in.*lbf
  No. 1 cooler refrigerant discharge hose x Cooler condenser assembly | 5.4 | 55 | 47 in.*lbf