GSIC - Global Service Information Center

### QUARTER WINDOW GLASS > REMOVAL

1. REMOVE FRONT SEAT ASSEMBLY (Bench Seat Type)

2. REMOVE FRONT SEAT ASSEMBLY (Separate Seat Type)

3. REMOVE FRONT DOOR SCUFF PLATE LH

4. REMOVE FRONT DOOR OPENING TRIM WEATHERSTRIP LH

5. REMOVE BACK PANEL GARNISH UPPER

6. REMOVE REAR SEAT CUSHION ASSEMBLY LH

7. REMOVE REAR SEAT CUSHION ASSEMBLY RH

8. REMOVE BACK PANEL GARNISH LOWER

9. REMOVE REAR SEATBACK ASSEMBLY

10. REMOVE FRONT SEAT OUTER BELT ASSEMBLY LH

11. REMOVE REAR NO. 1 SEAT BELT ASSEMBLY OUTER LH

12. REMOVE QUARTER INSIDE TRIM BOARD LH

13. REMOVE QUARTER PILLAR GARNISH LH

14. REMOVE ROOF SIDE GARNISH INNER UPPER LH

15. REMOVE QUARTER WINDOW ASSEMBLY LH