GSIC - Global Service Information Center

### CLUTCH UNIT > INSTALLATION

1. INSTALL INPUT SHAFT FRONT BEARING

2. INSTALL CLUTCH DISC ASSEMBLY

3. INSTALL CLUTCH COVER ASSEMBLY

4. INSPECT AND ADJUST CLUTCH COVER ASSEMBLY

5. INSTALL RELEASE FORK SUPPORT

6. INSTALL RELEASE BEARING HUB CLIP

7. INSTALL CLUTCH RELEASE FORK SUB-ASSEMBLY

8. INSTALL CLUTCH RELEASE BEARING ASSEMBLY

9. INSTALL CLUTCH RELEASE FORK BOOT

10. INSTALL MANUAL TRANSMISSION UNIT ASSEMBLY

11. INSTALL FRONT PROPELLER SHAFT ASSEMBLY (4WD)

12. INSTALL REAR PROPELLER SHAFT ASSEMBLY

13. INSTALL NO. 1 ENGINE COVER SUB-ASSEMBLY (4WD)

14. INSTALL NO. 2 ENGINE COVER SUB-ASSEMBLY (4WD)

15. CONNECT CABLE TO NEGATIVE BATTERY TERMINAL

16. PERFORM INITIALIZATION

17. CHECK SRS WARNING LIGHT