GSIC - Global Service Information Center

### DTC 62-42 Disc cannot be Read (AUDIO H/U)

### DTC 62-44 CD Abnormal (AUDIO H/U)

## for Preparation Click here

## DESCRIPTION

DTC No. | DTC Detection Condition | Trouble Area

62-42

Disc cannot be read.

1. CD
2. Radio receiver assembly

62-44 | Error is detected in CD player.

## INSPECTION PROCEDURE

1.CHECK IF PROPER CD IS INSERTED

1. Make sure that the CD is a normal audio CD, and that it is not deformed, flawed, stained, burred or otherwise defective.

   OK:
     Normal audio CD.

   HINT:
     Translucent or uniquely-shaped CDs cannot be played.

| NG |

CD IS FAULTY

OK |

2.CHECK THAT CD IS INSERTED PROPERLY

1. Check whether or not the CD is inserted upside down.

   OK:
     CD is properly inserted.

| NG |

INSERT CD PROPERLY

OK |

3.CLEAN CD

1. Clean the disc by wiping the CD's underside radially with a soft cloth.

   OK:
     Malfunction disappears.

   NOTICE:
     Do not use a conventional record cleaner or anti-static preservative.

| OK |

CD WAS DIRTY

NG |

REPAIR RADIO RECEIVER ASSEMBLY