GSIC - Global Service Information Center

### REAR LEAF SPRING (for 2WD) > REMOVAL

1. REMOVE REAR WHEEL

2. DISCONNECT NO. 3 PARKING BRAKE CABLE ASSEMBLY

3. REMOVE REAR SHOCK ABSORBER ASSEMBLY

4. REMOVE REAR LEAF SPRING BUMPER

5. REMOVE REAR LEAF SPRING U BOLT

6. REMOVE REAR LEAF SPRING BRACKET PIN OR PIN BOLT

7. REMOVE LEAF SPRING SHACKLE INNER PLATE

8. REMOVE NO. 2 REAR LEAF SPRING SHACKLE SUB-ASSEMBLY

9. REMOVE REAR LH LEAF SPRING ASSEMBLY