GSIC - Global Service Information Center

### AUDIO AND VISUAL SYSTEM > CD Sound Skips

## for Preparation Click here

## INSPECTION PROCEDURE

1.CLEAN CD

1. If the disc is dirty, clean the disc by wiping the CD's underside radially with a soft cloth.

   OK:
     Malfunction disappears.

   NOTICE:
     Do not use a conventional record cleaner or anti-static preservative.

| OK |

CD WAS DIRTY

NG |

2.REPLACE CD WITH ANOTHER AND RECHECK

1. Replace the CD with a normal one and check if the same problem occurs again.

   OK:
     Malfunction disappears.

| OK |

CD IS FAULTY

NG |

3.CHECK WHEN PROBLEM OCCURS

1. Check the location in which CD skipping occurs.

   Result
   Result | Proceed to
   Driving surface is bumpy or rough | A
   Driving surface is normal | B

| NG |

Go to step 5

OK |

4.CHECK RADIO RECEIVER ASSEMBLY INSTALLATION

1. Check the installation condition of the radio receiver.

   OK:
     Installed properly.

| NG |

INSTALL RADIO RECEIVER ASSEMBLY PROPERLY

OK |

5.COMPARE IT WITH ANOTHER VEHICLE OF SAME MODEL

1. Remove the radio receiver and install it in another vehicle of the same model. Check if the CD sound skips.

   OK:
     CD sound does not skip.

| OK |

MALFUNCTIONS MAY NOT BE PRESENT

NG |

6.DID TEMPERATURE IN CABIN CHANGE RAPIDLY?

1. Check whether or not a rapid temperature change occurred in the cabin.

   OK:
     Rapid temperature change occurred.

   HINT:
     A rapid temperature change creates condensation inside the CD player, which may disable CD playback.

| NG |

PROCEED TO NEXT CIRCUIT INSPECTION SHOWN IN PROBLEM SYMPTOMS TABLE

OK |

CONDENSATION DUE TO TEMPERATURE CHANGE (LEAVE AS IS FOR AWHILE BEFORE USING)