GSIC - Global Service Information Center

### LOAD SENSING PROPORTIONING VALVE > INSTALLATION

1. INSTALL LOAD SENSING PROPORTIONING VALVE ASSEMBLY

2. CONNECT NO. 2 LOAD SENSING SPRING SHACKLE

3. FILL RESERVOIR WITH BRAKE FLUID

4. BLEED AIR FROM BRAKE MASTER CYLINDER

5. BLEED AIR FROM BRAKE LINE

6. BLEED AIR FROM CLUTCH LINE (M/T)

7. CHECK BRAKE FLUID LEVEL IN RESERVOIR

8. CHECK FOR BRAKE FLUID LEAKAGE

9. CHECK LOAD SENSING PROPORTIONING VALVE ASSEMBLY

10. ADJUST LOAD SENSING PROPORTIONING VALVE ASSEMBLY