GSIC - Global Service Information Center

# AUDIO AND VISUAL SYSTEM > DIAGNOSTIC TROUBLE CODE CHART

## for Preparation Click here

RADIO RECEIVER ASSEMBLY (AUDIO H / U)
DTC No. | Detection Item | Suspected area | See page
01-D6 | No Master (AUDIO H/U) | Radio Receiver Assembly Wire Harness | Click here
01-D8 | No Response for Connection Check (AUDIO H/U) | Radio Receiver Assembly | Click here
01-D9 | Last Mode Error (AUDIO H/U) | Radio Receiver Assembly Wire Harness | Click here
01-DA | No Response Against ON / OFF Command (AUDIO H/U) | Radio Receiver Assembly Wire Harness | Click here
01-DB | Mode Status Error (AUDIO H/U) | Radio Receiver Assembly Wire Harness | Click here
01-DC | Failure in Transmission (AUDIO H/U) | Radio Receiver Assembly Wire Harness | Click here
01-DD | Master Reset (AUDIO H/U) | Radio Receiver Assembly Wire Harness | Click here
01-DE | Slave Reset (AUDIO H/U) | Radio Receiver Assembly Wire Harness | Click here
01-E0 | Registration Complete Indication Error (AUDIO H/U) | - | Click here
01-E2 | ON / OFF Indication Parameter Error (AUDIO H/U) | Radio Receiver Assembly | Click here
01-E3 | Registration Demand Transmission (AUDIO H/U) | - | Click here
01-E4 | Multiple Frame Incomplete (AUDIO H/U) | - | Click here
61-40 | Mechanical Error of Media (AUDIO H/U) | Cassette Tape Radio Receiver Assembly | Click here
62-42 | Disc cannot be Read (AUDIO H/U) | CD Radio Receiver Assembly | Click here
62-44 | CD Abnormal (AUDIO H/U) | CD Radio Receiver Assembly | Click here
62-45 | EJECT Error (AUDIO H/U) | CD Radio Receiver Assembly | Click here
62-46 | Disc Has Scratches in the Reverse Surface (AUDIO H/U) | CD Radio Receiver Assembly | Click here
62-47 | CD Temperature is High (AUDIO H/U) | Radio Receiver Assembly | Click here
62-48 | Excess Circuit (AUDIO H/U) | Radio Receiver Assembly | Click here
63-42 | Disc cannot be Read | CD Radio Receiver Assembly | Click here
63-44 | CD Abnormal | CD Radio Receiver Assembly | Click here
63-45 | Eject Error | CD Radio Receiver Assembly | Click here
63-46 | Scratched / Reversed Disc | CD Radio Receiver Assembly | Click here
63-47 | High Temperature | Radio Receiver Assembly | Click here
63-48 | Excess Current | Radio Receiver Assembly | Click here
63-51 | Elevator Error | Radio Receiver Assembly | Click here
63-52 | Clamp Error | Radio Receiver Assembly | Click here