GSIC - Global Service Information Center

### FRONT BRAKE FLEXIBLE HOSE > INSTALLATION

1. INSTALL FRONT FLEXIBLE HOSE (2WD)

2. INSTALL FRONT NO. 1 WHEEL CYLINDER TUBE LH (4WD)

3. INSTALL FRONT FLEXIBLE HOSE (4WD)

4. FILL RESERVOIR WITH BRAKE FLUID

5. BLEED AIR FROM BRAKE MASTER CYLINDER

6. BLEED AIR FROM BRAKE LINE

7. BLEED AIR FROM CLUTCH LINE (M/T)

8. CHECK BRAKE FLUID LEVEL IN RESERVOIR

9. CHECK FOR BRAKE FLUID LEAKAGE

10. INSTALL FRONT WHEEL