GSIC - Global Service Information Center

# VF2A TRANSFER > TORQUE SPECIFICATIONS

Transfer oil:

  Part tightened | N*m | kgf*cm | ft.*lbf
  No. 1 transfer case plug (filler and drain) x Transfer assembly | 37 | 377 | 27

Transfer case oil seal:

  Part tightened | N*m | kgf*cm | ft.*lbf
  Lower transfer case protector x Transfer assembly | 18 | 183 | 13

Extension housing oil seal:

  Part tightened | N*m | kgf*cm | ft.*lbf
  Lower transfer case protector x Transfer assembly | 18 | 183 | 13

Transfer assembly:

  Part tightened | N*m | kgf*cm | ft.*lbf
  Transfer case plug x Front transfer case | 18.6 | 190 | 14
  Transfer oil pump body sub-assembly x Front transfer case | 7.5 | 76 | 66 in.*lbf
  Transfer oil separator sub-assembly x Front transfer case | 7.5 | 76 | 66 in.*lbf
  No. 1 transfer case plug (filler and drain) x Transfer assembly | 37 | 377 | 27
  Rear transfer case x Front transfer case | 28 | 285 | 21
  Transfer extension housing sub-assembly x Rear transfer case | 12 | 22 | 9
  Transfer output shaft companion flange (front and rear) | 118 | 1,203 | 87
  Transfer control shift lever retainer sub-assembly x Front transfer case | 18 | 183 | 13
  Transfer case cover sub-assembly x Front transfer case | 18 | 183 | 13
  Transfer bearing retainer sub-assembly x Front transfer case | 11.5 | 117 | 8
  Transfer indicator switch x Front transfer case | 37 | 377 | 27
  Transfer assembly x Transmission assembly | 24 | 244 | 17
  Lower transfer case protector x Transfer assembly | 18 | 183 | 13

Speedometer driven gear:

  Part tightened | N*m | kgf*cm | ft.*lbf
  Vehicle speed sensor x Transfer extension housing sub-assembly | 11.5 | 117 | 8