GSIC - Global Service Information Center

### FUEL INJECTOR > INSTALLATION

1. INSTALL INJECTOR ASSEMBLY

2. CHECK FOR FUEL LEAKS

3. INSTALL CYLINDER HEAD COVER SUB-ASSEMBLY

4. INSTALL INJECTION PIPE

5. INSTALL CHARGE AIR COOLER ASSEMBLY WITH INTAKE AIR CONNECTOR

6. INSTALL NO. 1 ENGINE COVER SUB-ASSEMBLY

7. ADD FUEL

8. TIGHTEN FUEL TANK CAP ASSEMBLY

9. BLEED AIR FROM FUEL SYSTEM

10. CONNECT CABLE TO NEGATIVE BATTERY TERMINAL

11. PERFORM INITIALIZATION

12. REGISTER INJECTOR COMPENSATION CODE

13. CHECK FOR FUEL LEAKS

14. CHECK FOR OIL LEAKS