GSIC - Global Service Information Center

# EXTERIOR > TORQUE SPECIFICATIONS

FRONT BUMPER:

  Part Tightened | N*m | kgf*cm | ft.*lbf
  Front bumper reinforcement x Body | 67 | 683 | 49

REAR BUMPER (FOR STEP TYPE):

  Part Tightened | N*m | kgf*cm | ft.*lbf
  Rear bumper arm x Body | 45 | 459 | 33
  Rear bumper bar x Rear bumper arm | 45 | 459 | 33

REAR BUMPER (FOR FLAT TYPE):

  Part Tightened | N*m | kgf*cm | ft.*lbf
  Rear bumper arm x Body | 45 | 459 | 33
  Rear bumper arm x Body | 45 | 459 | 33

SIDE STEP:

  Part Tightened | N*m | kgf*cm | ft.*lbf
  Side step stay x Body | 18 | 184 | 13