GSIC - Global Service Information Center

# METER / GAUGE SYSTEM > PROBLEM SYMPTOMS TABLE

## for Preparation Click here

HINT:

1. Use the table below to help determine the cause of the problem symptom. The potential causes of the symptoms are listed in order of probability in the "Suspected area" column of the table. Check each symptom by checking the suspected area in the order they are listed. Replace parts as necessary.
2. Inspect the related fuses and relays before confirming the suspected area in the table below.

Malfunction system
Symptom | Suspected area | See page
Entire combination meter does not operate | Refer to troubleshooting | Click here
Operating light control rheostat does not change light brightness | Light control rheostat | -
Wire harness | -
Combination meter assembly | Click here

Meter gauges
Symptom | Suspected area | See page
Malfunction in speedometer | Refer to troubleshooting | Click here
Malfunction in tachometer | Refer to troubleshooting | Click here
Malfunction in fuel receiver gauge | Refer to troubleshooting | Click here
Malfunction in water temperature receiver gauge | Refer to troubleshooting | Click here

Warning lights
Symptom | Suspected area | See page
MIL does not turn on | Refer to troubleshooting (1TR-FE) | Click here
Refer to troubleshooting (2TR-FE) | Click here
Refer to troubleshooting (1GR-FE) | Click here
Refer to troubleshooting (1KD-FTV) | Click here
Refer to troubleshooting (2KD-FTV) | Click here
Discharge warning light does not turn on | Generator assembly (1TR-FE) | Click here
Generator assembly (2TR-FE) | Click here
Generator assembly (1GR-FE) | Click here
Generator assembly (1KD-FTV) | Click here
Generator assembly (2KD-FTV) | Click here
Wire harness | -
Combination meter assembly | Click here
Brake warning light does not turn on | Brake fluid level warning switch | Click here
Parking brake switch assembly | Click here
Vacuum warning switch | Click here
Wire harness | -
Combination meter assembly | Click here
ABS warning light does not turn on | Refer to troubleshooting | Click here
SRS warning light does not turn on | Refer to troubleshooting | Click here
Open door warning does not turn on | Door control light switch assembly | Click here
Wire harness | -
Combination meter assembly | Click here
Fuel level warning light does not turn on | Fuel suction w/ pump and gauge tube assembly | -
Wire harness | -
Combination meter assembly | Click here
Low oil pressure warning light does not turn on | Oil pressure switch assembly | -
Wire harness | -
Combination meter assembly | Click here
T-BELT warning light does not turn on | Combination meter assembly | Click here
ATF temperature warning does not turn on | Wire harness | -
TCM | -
Combination meter assembly | Click here
A/T P warning light does not turn on | Refer to troubleshooting | Click here
Seat belt warning light for driver side does not operate | Refer to troubleshooting | Click here
Fuel system warning light does not turn on | Wire harness | -
Fuel filter assembly | Click here
Combination meter assembly | Click here

Indicator lights
Symptom | Suspected area | See page
Turn indicator light does not turn on | Headlight dimmer switch assembly (turn signal switch) | Click here
Turn signal flasher relay | -
Wire harness | -
Combination meter assembly | Click here
HI BEAM indicator light does not turn on | Headlight dimmer switch assembly | Click here
Wire harness | -
Combination meter assembly | Click here
Taillight indicator light does not turn on | Headlight dimmer switch assembly | Click here
Wire harness | -
Combination meter assembly | Click here
Glow indicator light does not turn on | ECM (1TR-FE) | Click here
ECM (2TR-FE) | Click here
ECM (1GR-FE) | Click here
ECM (1KD-FTV) | Click here
ECM (2KD-FTV) | Click here
Wire harness | -
Combination meter assembly | Click here
4WD indicator light does not turn on | 4WD control ECU | -
Wire harness | -
Combination meter assembly | Click here
Cruise indicator light does not turn on | Refer to troubleshooting | Click here

Warning buzzer
Symptom | Suspected area | See page
Key reminder warning buzzer does not sound | Refer to troubleshooting | Click here
Light reminder warning buzzer does not sound | Refer to troubleshooting | Click here
Seat belt warning buzzer does not sound | Refer to troubleshooting | Click here

Accessory meter (multi-display)
Symptom | Suspected area | See page
Displays driving range value is not normal | Wire harness | -
Fuel injector assembly (1TR-FE) | Click here
Fuel injector assembly (2TR-FE) | Click here
Fuel injector assembly (1GR-FE) | Click here
ECM (1KD-FTV) | Click here
ECM (2KD-FTV) | Click here
Accessory meter assembly (multi-display) | -
Combination meter assembly | Click here
Displays average fuel consumption and instantaneous fuel consumption values are not normal | Wire harness | -
Accessory meter assembly (multi-display) | -
ECM (1KD-FTV) | Click here
ECM (2KD-FTV) | Click here
Fuel injector assembly (1TR-FE) | Click here
Fuel injector assembly (2TR-FE) | Click here
Fuel injector assembly (1GR-FE) | Click here
Combination meter assembly | Click here
Display does not operate at all | Accessory meter assembly (multi-display) | -
Outside temperature is not displayed | A/C ambient temperature sensor | Click here
Wire harness | -
Accessory meter assembly (multi-display) | -
Displays driving time is not normal | Accessory meter assembly (multi-display) | -
Compass function does not operate normally | Accessory meter assembly (multi-display) | -
Displays average vehicle speed value is not normal | Accessory meter assembly (multi-display) | -
Wire harness | -
Combination meter assembly | Click here
Seat belt warning light for passenger side does not blink | Refer to troubleshooting | Click here