GSIC - Global Service Information Center

# 1TR-FE FUEL > TORQUE SPECIFICATIONS

Part Tightened | N*m | kgf*cm | ft.*lbf
Fuel delivery pipe x Cylinder head | 12 | 122 | 9
Intake air connector x Cylinder head cover | 8.0 | 82 | 71 in.*lbf
Intake air connector x Hose clamp | 5.0 | 51 | 44 in.*lbf
Fuel pressure regulator x Fuel delivery pipe | 8.5 | 87 | 75 kgf*cm
Fuel filter x Body | 8.5 | 87 | 75 in.*lbf
Fuel tank band x Body | 61 | 622 | 54
Fuel tank filler pipe x Body | 19 | 194 | 14