GSIC - Global Service Information Center

### LOWER INSTRUMENT PANEL > REMOVAL

1. TABLE OF BOLT, SCREW AND NUT

2. DISCONNECT CABLE FROM NEGATIVE BATTERY TERMINAL

3. REMOVE INSTRUMENT PANEL SUB-ASSEMBLY UPPER

4. REMOVE WINDSHIELD WIPER SWITCH ASSEMBLY

5. REMOVE HEADLIGHT DIMMER SWITCH ASSEMBLY

6. REMOVE INSTRUMENT PANEL FINISH PANEL SUB-ASSEMBLY LOWER

7. REMOVE SHIFT LEVER KNOB SUB-ASSEMBLY

8. REMOVE PARKING BRAKE HOLE COVER SUB-ASSEMBLY

9. REMOVE CONSOLE PANEL SUB-ASSEMBLY UPPER

10. REMOVE CONSOLE BOX ASSEMBLY

11. REMOVE NO. 1 INSTRUMENT PANEL BOX

12. REMOVE SWITCH BASE

13. REMOVE FRONT DOOR SCUFF PLATE LH

14. REMOVE FRONT DOOR SCUFF PLATE RH

15. REMOVE COWL SIDE TRIM BOARD LH

16. REMOVE COWL SIDE TRIM BOARD RH

17. REMOVE INSTRUMENT PANEL SUB-ASSEMBLY LOWER