GSIC - Global Service Information Center

# ELECTRONIC CONTROLLED AUTOMATIC TRANSMISSION SYSTEM > DIAGNOSTIC TROUBLE CODE CHART

## for Preparation Click here

If a DTC is displayed during the DTC check, check the circuit listed in the table below and proceed to the page given.

HINT:

1. *1: "Comes on" means that the MIL will illuminate.
2. *2: "DTC stored" means that the ECM memorizes the malfunction code if the DTC detection condition(s) are met.
3. These DTCs may be output when the clutch, brake and gear components, etc., inside the automatic transmission are damaged.

AUTOMATIC TRANSMISSION SYSTEM
DTC No. | Detection Item | Trouble Area | MIL *1 | Memory *2 | See page
P0705 | Transmission Range Sensor Circuit Malfunction (PRNDL Input) | - Open or short in park/neutral position switch circuit - Park/neutral position switch - ECM | Comes on | DTC stored | Click here
P0710 | Transmission Fluid Temperature Sensor "A" Circuit | - Open or short in No. 1 ATF temperature sensor circuit - No. 1 ATF temperature sensor - ECM | Comes on | DTC stored | Click here
P0711 | Transmission Fluid Temperature Sensor "A" Performance | - No. 1 ATF temperature sensor | Comes on | DTC stored | Click here
P0712 | Transmission Fluid Temperature Sensor "A" Circuit Low Input | - Short in No. 1 ATF temperature sensor circuit - No. 1 ATF temperature sensor - ECM | Comes on | DTC stored | Click here
P0713 | Transmission Fluid Temperature Sensor "A" Circuit High Input | - Open in No. 1 ATF temperature sensor circuit - No. 1 ATF temperature sensor - ECM | Comes on | DTC stored | Click here
P0717 | Input Speed Sensor Circuit No Signal | - Open or short in speed sensor (NT) circuit - Input speed sensor (NT) - ECM - Automatic transmission (clutch, brake or gear, etc.) | Comes on | DTC stored | Click here
P0722 | Output Speed Sensor Circuit No Signal | - Open or short in speed sensor (SP2) circuit - Output speed sensor (SP2) - ECM - Automatic transmission (clutch, brake or gear, etc.) | Comes on | DTC stored | Click here
P0724 | Brake Switch "B" Circuit High | - Short in stop light switch signal circuit - Stop light switch - ECM | Comes on | DTC stored | Click here
P0748 | Pressure Control Solenoid "A" Electrical (Shift Solenoid Valve SL1) | - Open or short in shift solenoid valve SL1 circuit - Shift solenoid valve SL1 - ECM | Comes on | DTC stored | Click here
P0751 | Shift Solenoid "A" Performance (Shift Solenoid Valve S1) | - Shift solenoid valve S1 remains open or closed - Valve body is blocked - Automatic transmission (clutch, brake or gear, etc.) | Comes on | DTC stored | Click here
P0756 | Shift Solenoid "B" Performance (Shift Solenoid Valve S2) | - Shift solenoid valve S2 remains open or closed - Valve body is blocked - Automatic transmission (clutch, brake or gear, etc.) | Comes on | DTC stored | Click here
P0771 | Shift Solenoid "E" Performance (Shift Solenoid Valve SR) | - Shift solenoid valve SR remains open or closed - Shift solenoid valve SL1 remains open or closed - Valve body is blocked - Automatic transmission (clutch, brake or gear, etc.) | Comes on | DTC stored | Click here
P0776 | Pressure Control Solenoid "B" Performance (Shift Solenoid Valve SL2) | - Shift solenoid valve SL2 remains open or closed - Valve body is blocked - Automatic transmission (clutch, brake or gear, etc.) | Comes on | DTC stored | Click here
P0778 | Pressure Control Solenoid "B" Electrical (Shift Solenoid Valve SL2) | - Open or short in shift solenoid valve SL2 circuit - Shift solenoid valve SL2 - ECM | Comes on | DTC stored | Click here
P0781 | 1-2 Shift (1-2 Shift Valve) | - Valve body is blocked up or stuck (1-2 shift valve) - Automatic transmission (clutch, brake or gear, etc.) | Comes on | DTC stored | Click here
P0818 | Driveline Disconnect Switch Input Circuit | - Short in transfer neutral position switch circuit - Transfer neutral position switch - ECM | Comes on | DTC stored | Click here
P0973 | Shift Solenoid "A" Control Circuit Low (Shift Solenoid Valve S1) | - Short in shift solenoid valve S1 circuit - Shift solenoid valve S1 - ECM | Comes on | DTC stored | Click here
P0974 | Shift Solenoid "A" Control Circuit High (Shift Solenoid Valve S1) | - Open in shift solenoid valve S1 circuit - Shift solenoid valve S1 - ECM | Comes on | DTC stored | Click here
P0976 | Shift Solenoid "B" Control Circuit Low (Shift Solenoid Valve S2) | - Short in shift solenoid valve S2 circuit - Shift solenoid valve S2 - ECM | Comes on | DTC stored | Click here
P0977 | Shift Solenoid "B" Control Circuit High (Shift Solenoid Valve S2) | - Open in shift solenoid valve S2 circuit - Shift solenoid valve S2 - ECM | Comes on | DTC stored | Click here
P0985 | Shift Solenoid "E" Control Circuit Low (Shift Solenoid Valve SR) | - Short in shift solenoid valve SR circuit - Shift solenoid valve SR - ECM | Comes on | DTC stored | Click here
P0986 | Shift Solenoid "E" Control Circuit High (Shift Solenoid Valve SR) | - Open in shift solenoid valve SR circuit - Shift solenoid valve SR - ECM | Comes on | DTC stored | Click here
P2714 | Pressure Control Solenoid "D" Performance (Shift Solenoid Valve SLT) | - Shift solenoid valve SLT remains open or closed - Valve body is blocked - Automatic transmission (clutch, brake or gear, etc.) | Comes on | DTC stored | Click here
P2716 | Pressure Control Solenoid "D" Electrical (Shift Solenoid Valve SLT) | - Open or short in shift solenoid valve SLT circuit - Shift solenoid valve SLT - ECM | Comes on | DTC stored | Click here
P2740 | Transmission Fluid Temperature Sensor "B" Circuit | - Open or short in No. 2 ATF temperature sensor circuit - No. 2 ATF temperature sensor - ECM | Comes on | DTC stored | Click here
P2742 | Transmission Fluid Temperature Sensor "B" Circuit Low Input | - Short in No. 2 ATF temperature sensor circuit - No. 2 ATF temperature sensor - ECM | Comes on | DTC stored | Click here
P2743 | Transmission Fluid Temperature Sensor "B" Circuit High Input | - Open in No. 2 ATF temperature sensor circuit - No. 2 ATF temperature sensor - ECM | Comes on | DTC stored | Click here

P2757

Torque Converter Clutch Pressure Control Solenoid Performance (Shift Solenoid Valve SLU)

- Shift solenoid valve SLU remains open or closed
- Valve body is blocked
- Torque converter clutch
- Automatic transmission (clutch, brake or gear, etc.)
- Line pressure is too low

Comes on

DTC stored

Click here

P2759 | Torque Converter Clutch Pressure Control Solenoid Control Circuit Electrical (Shift Solenoid Valve SLU) | - Open or short in shift solenoid valve SLU circuit - Shift solenoid valve SLU - ECM | Comes on | DTC stored | Click here
P2772 | Transfer "L4" Switch Circuit | - Short in transfer L4 position switch circuit - Transfer L4 position switch - ECM | Comes on | DTC stored | Click here