GSIC - Global Service Information Center

### AUDIO AND VISUAL SYSTEM > Cassette Tape cannot be Inserted or Played

## for Preparation Click here

## INSPECTION PROCEDURE

1.CHECK FOR FOREIGN OBJECT

1. Check that the radio receiver cassette tape player is free from foreign objects.

   OK:
     No foreign objects.

| NG |

REMOVE FOREIGN OBJECT

OK |

2.CHECK CASSETTE TAPE

1. Check that the cassette tape is a normal tape for recording sounds.

   OK:
     Cassette tape is normal.

| NG |

CASSETTE TAPE IS FAULTY

OK |

3.REPLACE CASSETTE TAPE WITH ANOTHER AND RECHECK

1. Replace the cassette tape with a normal one and check if the same problem occurs again.

   OK:
     Same problem does not occur.

| NG |

PROCEED TO NEXT CIRCUIT INSPECTION SHOWN IN PROBLEM SYMPTOMS TABLE

OK |

CASSETTE TAPE IS FAULTY