GSIC - Global Service Information Center

### RADIATOR > INSTALLATION

1. INSTALL RADIATOR ASSEMBLY

2. INSTALL FAN SHROUD

3. CONNECT NO. 1 OIL COOLER INLET TUBE (for Automatic Transmission)

4. CONNECT NO. 1 OIL COOLER OUTLET TUBE (for Automatic Transmission)

5. CONNECT RADIATOR HOSE INLET

6. CONNECT RADIATOR HOSE OUTLET

7. CONNECT CABLE TO NEGATIVE BATTERY TERMINAL

8. ADD ENGINE COOLANT

9. CHECK FOR ENGINE COOLANT LEAKS

10. INSTALL RADIATOR SIDE DEFLECTOR RH

11. INSTALL RADIATOR SIDE DEFLECTOR LH

12. INSTALL RADIATOR GRILLE

13. INSTALL NO. 1 ENGINE UNDER COVER