GSIC - Global Service Information Center

# AIRBAG SYSTEM > DATA LIST / ACTIVE TEST

## for Preparation Click here

READ DATA LIST

HINT:

  Using the intelligent tester Data List allows switch, sensor, actuator and other item values to be read without removing any parts. Reading the Data List early in troubleshooting is one way to save time.

1. Connect the intelligent tester to the DLC3.

2. Turn the ignition switch ON.

3. Read the Data List according to the display on the tester.

   Airbag ECU:
   Item | Measurement Item/ Range (Display) | Normal Condition | Diagnostic Note
   Display Type Information | Display type identification information/ LR: Display is indicated by LH/RH DP: Display is indicated by Driver/Passenger | DP / LR | -
   Number of Past DTC | Number of past DTCs recorded/ Min.: 0, Max.: 255 | 0 | -