GSIC - Global Service Information Center

# SEAT BELT WARNING SYSTEM > PROBLEM SYMPTOMS TABLE

## for Preparation Click here

HINT:

  Use the table below to help determine the cause of the problem symptom. The potential causes of the symptoms are listed in order of probability in the "Suspected Area" column of the table. Check each symptom by checking the suspected areas in the order they are listed. Replace parts as necessary.

Symptom | Suspected area | See page
Driver seat belt warning light does not blink (ignition switch is ON and driver side buckle switch is ON (seat belt unfastened)) | MET fuse | Click here
Front seat inner belt assembly (driver side) | Click here
Combination meter assembly | Click here
Wire harness |
Passenger seat belt warning light does not blink (ignition switch is ON, occupant detection sensor is ON and passenger side buckle switch is ON (seat belt unfastened)) | ECU-IG & GAUGE fuse | Click here
Front seat inner belt assembly (passenger side) | Click here
Occupant detection sensor | Click here
Accessory meter assembly | Click here
Wire harness |