GSIC - Global Service Information Center

### OVERDRIVE DIRECT CLUTCH > DISASSEMBLY

1. INSPECT OVERDRIVE ONE-WAY CLUTCH

2. REMOVE OVERDRIVE DIRECT CLUTCH DRUM

3. INSPECT OVERDRIVE DIRECT CLUTCH DRUM

4. INSPECT PISTON STROKE OF OVERDRIVE DIRECT CLUTCH

5. REMOVE OVERDRIVE DIRECT CLUTCH DISC

6. INSPECT OVERDRIVE DIRECT CLUTCH DISC

7. REMOVE OVERDRIVE DIRECT CLUTCH RETURN SPRING

8. INSPECT OVERDRIVE DIRECT CLUTCH RETURN SPRING

9. REMOVE OVERDRIVE DIRECT CLUTCH PISTON

10. INSPECT OVERDRIVE DIRECT CLUTCH PISTON

11. REMOVE OVERDRIVE PLANETARY RING GEAR FLANGE

12. REMOVE OVERDRIVE RETAINING PLATE

13. REMOVE OVERDRIVE ONE-WAY CLUTCH OUTER RACE

14. REMOVE OVERDRIVE ONE-WAY CLUTCH

15. REMOVE NO.3 OVERDRIVE PLANETARY GEAR THRUST WASHER

16. INSPECT OVERDRIVE PLANETARY GEAR