GSIC - Global Service Information Center

# LICENSE PLATE LIGHT ASSEMBLY > INSTALLATION

## for Preparation Click here

1. INSTALL LICENSE PLATE LIGHT BULB

1. Install the bulb to the socket.

1. Turn the bulb/socket unit in the direction indicated by the arrow to install it.

2. INSTALL LICENSE PLATE LIGHT ASSEMBLY

1. Attach the license plate light with the 2 claws.

1. Connect the connector.

3. CONNECT CABLE TO NEGATIVE BATTERY TERMINAL

4. PERFORM INITIALIZATION

1. Perform initialization (Click here ).

   NOTICE:
     Certain systems need to be initialized after disconnecting and reconnecting the cable from the negative (-) battery terminal.