GSIC - Global Service Information Center

# VALVE BODY ASSEMBLY > DISASSEMBLY

## for Preparation Click here

1. REMOVE SHIFT SOLENOID VALVE

1. Remove the bolt, lock plate, 2 pins and shift solenoid valve SLT and SL1.

1. Remove the bolt, lock plate, 2 pins and shift solenoid valves SLU and SL2.

1. Remove the 2 bolts and shift solenoid valve SR.

1. Remove the bolt and shift solenoid valve S1.

1. Remove the bolt and shift solenoid valve S2.