GSIC - Global Service Information Center

# DOOR CONTROL TRANSMITTER MODULE > REMOVAL

1. REMOVE TRANSMITTER HOUSING COVER

NOTICE:

  Take extra care when handling these precision electronic components.

1. Twist the screwdriver in the direction of the arrow mark in the illustration, and open the transmitter housing cover.

   NOTICE:
     Do not forcibly pry the cover.

   HINT:
     Tape the screwdriver tip before use.

2. REMOVE DOOR CONTROL TRANSMITTER MODULE

1. Detach the hook of the transmitter battery's cover and remove the cover.