GSIC - Global Service Information Center

# AIR CONDITIONING AND BLOWER UNIT > REASSEMBLY

## for Preparation Click here

1. INSTALL BLOWER WITH FAN MOTOR SUB-ASSEMBLY

1. Install the blower motor with the 3 screws.

2. INSTALL BLOWER RESISTOR

1. Install the blower resistor with the 2 screws.

3. INSTALL MODE CONTROL CABLE SUB-ASSEMBLY

1. Attach the 3 claws and install the cable.

4. INSTALL AIR INLET DAMPER CONTROL CABLE SUB-ASSEMBLY

1. Attach the 3 claws and install the cable.

5. INSTALL NO. 3 AIR DUCT

1. Attach the 4 claws and install the duct.