GSIC - Global Service Information Center

# 1TR-FE IGNITION > TORQUE SPECIFICATIONS

Part Tightened | N*m | kgf*cm | ft.*lbf
Spark plug x Cylinder head | 18 | 183 | 13
Ignition coil x Cylinder head cover | 9.0 | 92 | 80 in.*lbf
Camshaft position sensor x Timing chain cover plate | 8.5 | 87 | 75 in.*lbf
Crankshaft position sensor x Timing chain cover plate | 8.5 | 87 | 75 in.*lbf
Cooler compressor assembly x No. 1 mounting bracket | 8.5 | 87 | 75 in.*lbf
Cylinder block x No. 1 mounting bracket | for bolt A | 24.5 | 250 | 18
for except bolt A | 45 | 459 | 33