GSIC - Global Service Information Center

# SIDE TURN SIGNAL LIGHT ASSEMBLY > INSTALLATION

## for Preparation Click here

1. INSTALL SIDE TURN SIGNAL LIGHT BULB

1. Install the bulb to the socket.

1. Turn the bulb/socket unit in the direction indicated by the arrow to install it.

2. INSTALL SIDE TURN SIGNAL LIGHT ASSEMBLY

1. Connect the connector and install the side turn signal light.

1. Attach the side turn signal light with the 2 claws and install the light as shown in the illustration.

3. CONNECT CABLE TO NEGATIVE BATTERY TERMINAL

4. PERFORM INITIALIZATION

1. Perform initialization (Click here ).

   NOTICE:
     Certain systems need to be initialized after disconnecting and reconnecting the cable from the negative (-) battery terminal.