GSIC - Global Service Information Center

# INSTRUMENT PANEL SAFETY PAD > DISASSEMBLY

## for Preparation Click here

1. REMOVE METER MOUNTING BRACKET

1. Remove the screw <B> and bracket.

2. REMOVE NO. 1 INSTRUMENT PANEL REGISTER ASSEMBLY

1. Detach the 4 claws and remove the register.

3. REMOVE NO. 2 INSTRUMENT PANEL REGISTER ASSEMBLY

HINT:

  Use the same procedures described for the No. 1 register.

4. REMOVE INSTRUMENT PANEL CUP HOLDER SUB-ASSEMBLY

1. Remove the 3 screws <B> and cup holder.