GSIC - Global Service Information Center

### OIL PUMP > DISASSEMBLY

1. REMOVE FRONT OIL PUMP BODY O-RING

2. FIX OIL PUMP ASSEMBLY

3. REMOVE CLUTCH DRUM OIL SEAL RING

4. REMOVE STATOR SHAFT ASSEMBLY

5. REMOVE FRONT OIL PUMP BODY O-RING

6. INSPECT FRONT OIL PUMP BODY SUB-ASSEMBLY

7. INSPECT STATOR SHAFT ASSEMBLY

8. INSPECT CLEARANCE OF OIL PUMP ASSEMBLY

9. REMOVE FRONT OIL PUMP DRIVE GEAR

10. REMOVE FRONT OIL PUMP DRIVEN GEAR

11. REMOVE FRONT OIL PUMP OIL SEAL