GSIC - Global Service Information Center

# POWER WINDOW CONTROL SYSTEM > PROBLEM SYMPTOMS TABLE

## for Preparation Click here

HINT:

1. Use the table below to help determine the cause of the problem symptom. The potential causes of the symptoms are listed in order of probability in the "Suspected Area" column of the table. Check each symptom by checking the suspected areas in the order they are listed. Replace parts as necessary.

1. Inspect the fuses and relays related to the system before inspecting the suspected areas below.

Power window control system
Symptom | Suspected area | See page
Remote Up / Down Function does not Operate | Power window regulator master switch assembly | Click here
Wire harness | Click here
Driver Side Power Window does not Operate with Power Window Master Switch | Power window regulator master switch assembly | Click here
Power window regulator motor assembly (driver side) | Click here
Wire harness | Click here
Front Passenger Side Power Window does not Operate with Front Passenger Side Power Window Switch | Power window regulator switch assembly (passenger side) | Click here
Power window regulator motor assembly (passenger side) | Click here
Wire harness | Click here
Rear Power Window LH does not Operate with Rear Power Window Switch LH* | Power window regulator switch assembly (rear LH)* | Click here
Power window regulator motor assembly (rear LH)* | Click here
Wire harness | Click here
Rear Power Window RH does not Operate with Rear Power Window Switch RH* | Power window regulator switch assembly (rear RH)* | Click here
Power window regulator motor assembly (rear RH)* | Click here
Wire harness | Click here
Power Windows do not Operate at All | ECU-IG & GAUGE fuse | Click here
IG1 relay | Click here
Power window regulator master switch assembly | Click here
Wire harness | Click here

HINT:

  *: Double cab