GSIC - Global Service Information Center

### ENGINE > ON-VEHICLE INSPECTION

1. INSPECT AIR CLEANER FILTER ELEMENT

2. INSPECT V-RIBBED BELT TENSIONER

3. INSPECT NO. 1 IDLER PULLEY

4. CHECK VALVE LASH ADJUSTER NOISE

5. INSPECT IGNITION TIMING

6. INSPECT ENGINE IDLE SPEED

7. INSPECT IDLE SPEED CONTROL SYSTEM

8. INSPECT COMPRESSION

9. CHECK CO (for Leaded Gasoline Specification Vehicle)

10. CHECK CO/HC (for Unleaded Gasoline Specification Vehicle)