GSIC - Global Service Information Center

### RADIATOR > INSTALLATION

1. INSTALL RADIATOR ASSEMBLY

2. INSTALL FAN SHROUD

3. CONNECT RADIATOR HOSE INLET

4. CONNECT RADIATOR HOSE OUTLET

5. CONNECT CABLE TO NEGATIVE BATTERY TERMINAL

6. ADD ENGINE COOLANT

7. CHECK FOR ENGINE COOLANT LEAKS

8. INSTALL RADIATOR SIDE DEFLECTOR LH

9. INSTALL RADIATOR SIDE DEFLECTOR RH

10. INSTALL RADIATOR GRILLE

11. INSTALL NO. 1 ENGINE UNDER COVER

12. PERFORM INITIALIZATION