GSIC - Global Service Information Center

# DIFFERENTIAL > TORQUE SPECIFICATIONS

FRONT DIFFERENTIAL CARRIER
Part tightened | N*m | kgf*cm | ft.*lbf
Differential breather hose x Differential carrier | 13 | 133 | 10
No. 3 differential support x No. 1 differential mount nut | 87 | 887 | 64
No. 3 differential support x Differential carrier | 108 | 1,100 | 80
No. 2 differential support x Differential carrier | 160 | 1,630 | 118
No. 1 differential support x Differential carrier | 186 | 1,900 | 137
Differential tube x Differential carrier | 110 | 1,120 | 81
Differential tube x Differential vacuum actuator | 21 | 210 | 15
Drive pinion companion flange x Drive pinion | 370 | 3,770 | 273
Differential side bearing retainer x Differential carrier | 50 | 510 | 37
Differential case x Differential rig gear | 97 | 985 | 71
Differential carrier x Drain lug | 65 | 660 | 48
Differential carrier x Filler plug | 39 | 400 | 29

REAR DIFFERENTIAL CARRIER
Part tightened | N*m | kgf*cm | ft.*lbf
Axle housing x Drain plug Axle housing x Filler plug | 49 | 500 | 36
Speed sensor x Backing plate | 8.0 | 82 | 71 in.*lbf
Brake liner x Backing plate | 15 | 155 | 11
Axle housing x Backing plate | 69 | 700 | 51
Axle housing x Differential carrier | 21 | 214 | 15
Differential carrier x Propeller shaft | 88 | 899 | 65
Drive pinion companion flange nut x Differential drive pinion | 370 | 3,770 | 273
Bearing cap x Differential bearing adjusting nut lock | 13 | 130 | 9
Differential case x Differential ring gear | 2 Pinion type: 84 LSD type: 47 | 2 Pinion type: 857 LSD type: 480 | 2 Pinion type: 62 LSD type: 35