GSIC - Global Service Information Center

# 2KD-FTV STARTING > TORQUE SPECIFICATIONS

Part Tightened | N*m | kgf*cm | ft.*lbf
Terminal 30 x Starter assembly | 9.8 | 100 | 87 in.*lbf
Terminal C x Starter assembly | 5.9 | 60 | 52 in.*lbf
Starter assembly x Transmission housing | 68 | 693 | 50
Glow plug x Cylinder head | 13 | 133 | 10
Glow plug connector x Glow plug (Nut) | 2.2 | 22 | 19 in.*lbf
Nut x Wire harness | 2.0 | 20 | 18 in.*lbf
Intake air connector x Intake manifold | 20 | 204 | 15
Throttle body bracket x Cylinder head | 20 | 204 | 15