GSIC - Global Service Information Center

# RADIO RECEIVER > INSTALLATION

## for Preparation Click here

1. INSTALL RADIO RECEIVER ASSEMBLY WITH BRACKET

1. w/ Stereo opening cover:
   Install the No. 1 radio bracket.

   1. Install the 4 screws and radio bracket to the radio receiver.

1. w/Stereo opening cover:
   Install the No. 2 radio bracket.

   1. Install the 4 screws and radio bracket to the radio receiver.

1. w/o Stereo opening cover:
   Install the No. 1 radio bracket.

   1. Install the 4 screws and radio bracket to the radio receiver.

1. w/o Stereo opening cover:
   Install No. 2 radio bracket.

   1. Install the 4 screws and radio bracket to the radio receiver.

1. Connect all connectors and install the radio receiver.

1. Install the radio receiver with the 4 screws.

2. INSTALL INSTRUMENT CLUSTER FINISH PANEL ASSEMBLY CENTER

1. Connect all connectors.

1. Attach the 6 claws and 4 clips to install the panel.

1. Install the panel with the screw <C>.

3. INSTALL FRE/REC CONTROL KNOB

1. Install the control knob.

4. INSTALL HEATER CONTROL KNOB

1. Install the 3 control knobs.

5. CONNECT CABLE TO NEGATIVE BATTERY TERMINAL

6. PERFORM INITIALIZATION

1. Perform initialization (Click here ).

   NOTICE:
     Certain systems need to be initialized after disconnecting and reconnecting the cable from the negative (-) battery terminal.