GSIC - Global Service Information Center

### CLUTCH MASTER CYLINDER > INSTALLATION

1. INSTALL CLUTCH MASTER CYLINDER ASSEMBLY

2. INSTALL CLUTCH MASTER CYLINDER TO FLEXIBLE TUBE

3. CONNECT CLUTCH RESERVOIR HOSE

4. INSTALL COMBINATION METER ASSEMBLY

5. INSTALL INSTRUMENT CLUSTER FINISH PANEL

6. BLEED AIR FROM CLUTCH PIPE LINE

7. CHECK FOR CLUTCH FLUID LEAKAGE

8. INSPECT AND ADJUST CLUTCH PEDAL ASSEMBLY

9. CHECK FLUID LEVEL IN RESERVOIR