GSIC - Global Service Information Center

### REAR SPEAKER (for Extra Cab) > INSTALLATION

1. INSTALL REAR NO. 1 SPEAKER ASSEMBLY

2. INSTALL QUARTER INSIDE TRIM BOARD

3. INSTALL REAR NO. 1 SEAT BELT ASSEMBLY OUTER LH

4. INSTALL FRONT SEAT OUTER BELT ASSEMBLY LH

5. INSTALL REAR SEATBACK ASSEMBLY

6. INSTALL BACK PANEL GARNISH LOWER

7. INSTALL REAR SEAT CUSHION ASSEMBLY LH

8. INSTALL REAR SEAT CUSHION ASSEMBLY RH

9. INSTALL BACK PANEL GARNISH UPPER

10. CONNECT CABLE TO NEGATIVE BATTERY TERMINAL

11. PERFORM INITIALIZATION