GSIC - Global Service Information Center

### BRAKE ACTUATOR > INSTALLATION

1. INSTALL BRAKE ACTUATOR ASSEMBLY WITH BRACKET

2. FILL RESERVOIR WITH BRAKE FLUID

3. BLEED AIR FROM BRAKE MASTER CYLINDER

4. BLEED AIR FROM BRAKE LINE

5. BLEED AIR FROM CLUTCH LINE (M/T)

6. CHECK BRAKE FLUID LEVEL IN RESERVOIR

7. CHECK FOR BRAKE FLUID LEAKAGE

8. CONNECT CABLE TO NEGATIVE BATTERY TERMINAL

9. CHECK BRAKE ACTUATOR WITH INTELLIGENT TESTER

10. PERFORM INITIALIZATION