GSIC - Global Service Information Center

### RADIATOR > INSTALLATION

1. INSTALL RADIATOR ASSEMBLY

2. CONNECT NO. 1 OIL COOLER TUBE INLET (for Automatic Transmission)

3. CONNECT NO. 1 OIL COOLER TUBE OUTLET (for Automatic Transmission)

4. INSTALL FAN SHROUD

5. CONNECT RADIATOR HOSE INLET

6. CONNECT RADIATOR HOSE OUTLET

7. ADD ENGINE COOLANT

8. CONNECT CABLE TO NEGATIVE BATTERY TERMINAL

9. CHECK FOR ENGINE COOLANT LEAKS

10. INSTALL RADIATOR SIDE DEFLECTOR LH

11. INSTALL RADIATOR SIDE DEFLECTOR RH

12. INSTALL RADIATOR GRILLE

13. INSTALL NO. 1 ENGINE UNDER COVER

14. PERFORM INITIALIZATION