GSIC - Global Service Information Center

### CAMSHAFT (for Bank 2) > INSTALLATION

1. INSTALL NO. 3 CAMSHAFT

2. INSTALL NO. 3 CHAIN TENSIONER

3. INSTALL NO. 4 CAMSHAFT

4. INSTALL NO. 1 CHAIN TENSIONER

5. SET NO. 1 CYLINDER TO TDC/COMPRESSION

6. INSPECT VALVE CLEARANCE

7. ADJUST VALVE CLEARANCE

8. INSTALL CYLINDER HEAD COVER LH

9. INSTALL CYLINDER HEAD COVER RH

10. INSTALL IGNITION COIL

11. INSTALL INTAKE AIR SURGE TANK

12. REMOVE AIR CLEANER

13. CONNECT NO. 2 VENTILATION HOSE

14. CONNECT CABLE TO BATTERY NEGATIVE TERMINAL

15. PERFORM INITIALIZATION

16. ADD ENGINE COOLANT

17. CHECK FOR ENGINE COOLANT LEAKS

18. INSTALL V-BANK COVER

19. INSPECT IGNITION TIMING