GSIC - Global Service Information Center

### DTC B2793 Transponder Chip Malfunction

## DESCRIPTION

This DTC is output when: 1) during key code registration, a key malfunction occurs; or 2) the key code was unable to be registered properly.

DTC No. | DTC Detection Condition | Trouble Area
B2793 | Transponder chip malfunction | Key

## INSPECTION PROCEDURE

1.REREGISTER KEY

1. Delete the DTC (Click here).

1. Reregister the key, and check that the engine starts with the key.

   OK:
     Engine starts.

| NG |

REPLACE KEY

OK |

NORMAL (INSPECTION FINISHED)