GSIC - Global Service Information Center

### AUDIO AND VISUAL SYSTEM > CD cannot be Ejected

## for Preparation Click here

## INSPECTION PROCEDURE

1.PRESS ''EJECT'' AND CHECK OPERATION

1. Press the CD EJECT switch of the radio receiver for 2 seconds or more and check that the CD ejects.

   OK:
     CD ejects.

| NG |

PROCEED TO NEXT CIRCUIT INSPECTION SHOWN IN PROBLEM SYMPTOMS TABLE

OK |

2.REPLACE CD WITH ANOTHER AND RECHECK

1. Replace the CD with a normal one and check that the CD ejects.

   OK:
     CD ejects.

| NG |

PROCEED TO NEXT CIRCUIT INSPECTION SHOWN IN PROBLEM SYMPTOMS TABLE

OK |

CD IS FAULTY